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WEEKLY JOBSITE SAFETY INSPECTION CHECKLIST

Note: The acting superintendent must conduct this dedicated jobsite safety inspection on a weekly basis and no other non-safety related items should be reviewed or addressed during this inspection.

	PROJECT NAME:                                                                             JOB #:

	PROJECT SUPERINTENDENT:

	DATE:

	INSPECTED BY (must be by acting Superintendent):


COLUMNS:
A – Satisfactory at time of inspection


B – Needs immediate attention


       
C – Needs further consideration 



D – Not Applicable


Check the appropriate column below based upon jobsite condition at time of inspection.

	SAFETY ITEM
	A
	B
	C
	D

	General – OHSA forms & jobsite warning signs posted
	
	
	
	

	     ME&S safety policy, first aid kit, and job-specific MSDS in jobsite office
	
	
	
	

	     ME&S onsite employees properly trained for jobsite tasks & equipment
	
	
	
	

	     Subcontractor-specific safety/fall protection plans onsite
	
	
	
	

	     Weekly safety meetings held and minutes maintained onsite
	
	
	
	

	Housekeeping – Jobsite neat & clean with materials stored properly
	
	
	
	

	     Walkways clear of debris and other trip/slip hazards
	
	
	
	

	     Adequate lighting to perform all required tasks
	
	
	
	

	     Drinking water provided incl. new cups and disposal area for used ones
	
	
	
	

	     Toilets provided and clean
	
	
	
	

	Fire Prevention – Fire extinguishers charged, proper number & locations
	
	
	
	

	     “No smoking” signs posted and enforced where needed
	
	
	
	

	     Flammable liquid containers UL or FM listed & clearly identified
	
	
	
	

	Electrical – GFCI breakers & sufficient number of temp outlets provided
	
	
	
	

	     Energized switchgear, panels & devices marked and/or guarded
	
	
	
	

	     Equipment grounded & non-spliced, non-damaged 3-prong cords used
	
	
	
	

	     Temp lights provided with guards to prevent accidental bulb contact 
	
	
	
	

	     Lock-out / Tag-out program utilized
	
	
	
	

	Hand & Power Tools – Cords in good condition (no frays or damage)
	
	
	
	

	     Tools in good condition with all safeguards in place and working
	
	
	
	

	     Proper tool being utilized for each task with properly trained employee
	
	
	
	

	Ladders & Stairways – Ladders in good condition (no paint or damage)
	
	
	
	

	     Side-rails extended at least 36” above top of landing or grab rails used
	
	
	
	

	     Rungs or cleats not spaced more than 12” on center
	
	
	
	

	     Ladders properly secured to prevent slipping, sliding or falling
	
	
	
	

	     Stepladders fully open when in use
	
	
	
	

	     No metal ladders utilized around electrical hazards
	
	
	
	

	     Ladder or stairs provided for access at any elevation change > 19”
	
	
	
	

	     Stairways have proper treads and railings and are properly lighted
	
	
	
	

	Heavy Equipment / Lifts – Operators properly trained & authorized
	
	
	
	

	     Signal horns and back-up alarms operational
	
	
	
	

	     Roll-over protection required and seat belts provided and worn
	
	
	
	

	     Workers in lift basket standing on floor or wearing fall protection equip
	
	
	
	

	     Seat belts worn while operating equipment
	
	
	
	

	     Chains connected across aerial lift openings at access side
	
	
	
	

	SAFETY ITEM
	A
	B
	C
	D

	Scaffolding – Erection/modification is/was properly supervised
	
	
	
	

	     Daily inspections conducted by respective subcontractor
	
	
	
	

	     Platforms 10’ above surface have 42” top rails, midrails, & 4” toeboards
	
	
	
	

	     Overhead protection provided for workers below
	
	
	
	

	     Access ladders properly provided
	
	
	
	

	     Planks undamaged and extend between 6” & 12” over supports
	
	
	
	

	     Scaffold tied to and braced against structure
	
	
	
	

	     Adequate foundation bearing plates with foot-sills and mudsills provided
	
	
	
	

	     Scaffolding plumb and square and all connections secure
	
	
	
	

	     Rolling scaffold – Height does not exceed 4 times least base dimension
	
	
	
	

	Fall Protection – Safety rails provided at all open-sided floors
	
	
	
	

	     Safety rails or covers provided at all floor openings/holes
	
	
	
	

	     Fall protection provided at surfaces 6’ or more above floor or ground
	
	
	
	

	     CAZs clearly marked with access allowed to authorized workers only
	
	
	
	

	     Warning lines for roofing CAZs not less than 6’ back from edge
	
	
	
	

	Personal Protective Equipment - Hard hats worn
	
	
	
	

	     Safety glasses & hearing protective devices utilized when required
	
	
	
	

	     Safety harnesses & lanyards utilized when required
	
	
	
	

	     Dust masks & respirators utilized when exposed to harmful dusts, etc.
	
	
	
	

	Personal Attire – Hard-soled ankle-high work boots, shirts and long pants
	
	
	
	

	Public Protection – Fencing provided / barricades around openings
	
	
	
	

	     Construction Site/No trespassing signs posted
	
	
	
	

	     Maintenance of traffic properly provided including flag person
	
	
	
	

	Compressed Gas Cylinders - Properly secured (upright) & properly

     separated (min. dist. of 20’ or 5’ high wall with ½ hour fire rating.)
	
	
	
	

	Concrete / Masonry – Vertical rebar protected by covering / flat caps
	
	
	
	

	     Shoring & re-shoring per drawings and adequate for support
	
	
	
	

	     Masonry walls properly supported to prevent overturn or collapse
	
	
	
	

	Excavations - Trenches properly excavated, shored, and barricaded
	
	
	
	

	     Excavated material effectively stored at least 2’ from edge of excavation
	
	
	
	

	     Excavations sloped or shored if 5’ in depth or deeper
	
	
	
	

	     Ladders provided every 25’ in trenches 4’ in depth or greater
	
	
	
	

	     Excavations inspected daily or more frequently if required (rain, etc.)
	
	
	
	

	     All utilities located and identified
	
	
	
	


Deficiencies noted above were corrected as follows (include date corrected):

Reviewed by Project Manager (sign here):





Date:
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